
INTERNATIONAL HYDROGRAPHIC ORGANIZATION



IHO UNIVERSAL HYDROGRAPHIC DATA MODEL

**Special Publication No. 127**

**Marine Traffic Management Product Specification**

**Version 1.0.1**

**Appendix E**

**Data Validation Checks**

Published by the

International Hydrographic Bureau

**MONACO**

|  |
| --- |
| © Copyright International Hydrographic Organization November 2019 |
| This work is copyright. Apart from any use permitted in accordance with the [Berne Convention for the Protection of Literary and Artistic Works](http://www.wipo.int/treaties/en/ip/berne/trtdocs_wo001.html) (1886), and except in the circumstances described below, no part may be translated, reproduced by any process, adapted, communicated or commercially exploited without prior written permission from the International Hydrographic Bureau (IHB). Copyright in some of the material in this publication may be owned by another party and permission for the translation and/or reproduction of that material must be obtained from the owner. |
| This document or partial material from this document may be translated, reproduced or distributed for general information, on no more than a cost recovery basis. Copies may not be sold or distributed for profit or gain without prior written agreement of the IHB and any other copyright holders. |
| In the event that this document or partial material from this document is reproduced, translated or distributed under the terms described above, the following statements are to be included: |
| *“Material from IHO publication [reference to extract: Title, Edition] is reproduced with the permission of the International Hydrographic Bureau (IHB) (Permission No ……./…) acting for the International Hydrographic Organization (IHO), which does not accept responsibility for the correctness of the material as reproduced: in case of doubt, the IHO’s authentic text shall prevail. The incorporation of material sourced from IHO shall not be construed as constituting an endorsement by IHO of this product.”* |
| *“This [document/publication] is a translation of IHO [document/publication] [name]. The IHO has not checked this translation and therefore takes no responsibility for its accuracy. In case of doubt the source version of [name] in [language] should be consulted.”*  The IHO Logo or other identifiers shall not be used in any derived product without prior written permission from the IHB. |

1. References

IHO S-58 ENC VALIDATION CHECKS Edition 6.1.0, September 2018

IHO S-97 Part C IHO data quality checklist [Draft 0.2, August 2018]

1. Abbreviation

PS – Product Specification

DCEG – Data Capture and Encoding Guide

1. Production validation checks for S-127 Marine Traffic Management

The following checks are intended for production systems designed to produce S-127 Marine Traffic Management datasets. The checks can be administered at any time during the production phase. All checks should be considered as warnings, even though more severe classifications are available, due to the status of the development and lack of experience with system use of S-127 datasets, it is considered premature to classify any checks as error or critical error at this time. All operators and spatial expressions are defined in Annex A.

* 1. Check classification

|  |  |  |
| --- | --- | --- |
| C | Critical Error | An error which would make an MTM dataset unusable in ECDIS through not loading or causing an ECDIS to crash or presenting data which is unsafe for navigation. |
| E | Error | An error which may degrade the quality of the MTM dataset through appearance or usability but which will not pose a significant danger when used to support navigation. |
| W | Warning | An error which may be duplication or an inconsistency which will not noticeably degrade the usability of an MTM dataset in ECDIS. |

* + 1. Check application

|  |  |  |
| --- | --- | --- |
| B | Base | Apply check to new dataset, new edition, and post-update dataset (after updates have been applied to the base). |
| U | Update | Apply check to update datasets in isolation. |
| S | Post-update | Apply check only to a post-update dataset, i.e., subsequent to application of all available updates. |

Checks do not apply to dataset terminations or cancellations, except where the check description explicitly states it applies in case of a termination or cancellation.

* 1. Checks relating to MTM Product Specification

[This table will be extended with indication of which of the data quality elements applies to each test after IHO S-97 Part C matures. The elements are described in Clause 9 of the main S-127 product specification.]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **No** | **Check description** | **Check message** | **Check solution** | **Conformity to** | **Apply to** |
| 100 | For each feature object where its geometry is not COVERED\_BY a DataCoverage | Objects fall outside the coverage object. | Ensure objects are not outside of the limits of the cell. | PS 10.9 | B, S |
| 101 | If the cell file size is greater than 20 Megabytes. | The cell is larger than 20Mb in size. | Ensure that the cell is not larger than 20Mb. | PS 11.2 | B, S |
| 102 | For each feature record where the name is not unique WITHIN the dataset. | Duplicate FOIDs exist within the dataset. | Ensure that no duplicate FOIDs exist. | PS 10.8 | B, U, S |
| 103 | If either QualityOfNonbathymetricData or DataCoverage meta feature objects do not exist within the data set. | Mandatory feature objects are missing. | Include mandatory meta feature objects QualityOfNonbathymetricData or DataCoverage. | PS 10.9 and 10.11 | B, S |
| 104 | If any mandatory attributes are not present. | Mandatory attributes are not encoded. | Populate mandatory attributes (If unknown encode attribute with empty value). | PS 10.5 | B, U |
| 105 | For each feature object with an attribute of type Float or Integer where the value contains zeroes before the first numerical digit or after the last numerical digit. | Values have been padded with non-significant zeroes. E.g. : For a signal frequency of 156.8 MHz, the value of SIGPER must be 156800000 and not 0156800000. | Remove non-significant zeroes. | PS 10.3 | B, U |
| 106 | For each feature object with an attribute value identical to a corresponding attribute of a meta feature object it is COVERED\_BY. | An attribute value of a meta feature object is duplicated on a geo object. | Remove duplicate value from geo object. | Logical consistency | B, S |
| 107 | For each association between features instances, features instances and information instances, and between information instances that is not defined in the feature catalogue. | Wrong association used. | Use correct association type. | Logical consistency | B, U |
| 108 | For each role name on associations that is not defined in the feature catalogue. | Wrong role used. | Use correct role name. | Logical consistency | B, U |
| 109 | For each association that is not defined in the feature catalogue. | Unknown association is used. | Use association that is defined in the feature catalogue. | Logical consistency | B, U |
| 110 | For each role name that is not defined in the feature catalogue. | Unknown role name is used. | Use role name that is defined in the feature catalogue. | Logical consistency | B, U |
| 111 | For each association ensure associated classes are only those permitted by the feature catalogue. | Class is associated in an illegal association. | Ensure correct association is used between classes. | Logical consistency | B, U, S |
| 112 | For each role name ensure it is only used with permitted associations. | Role name is used on an illegal association. | Ensure correct role names are used on the association. | Logical consistency | B, U, S |
| 113 | Ensure dataset conformance to the GML schema. | Dataset does not conform to the GML schema. | Ensure conformance to the GML schema. | PS 10.1.1 & 11.1 | B, U |
| 114 | Ensure all text fields are encoded using UTF-8. | Illegal character set used. | Change character encoding to UTF-8. | PS 10.4 | B, U |
| 115 | For each feature instance where more than one featureName is present, and the name subattribute of two or more featureName instances is equal. | Values name sub attribute are identical. | Ensure that name subattributes are populated with the correct values. | Logical consistency | B, U |
| 116 | For each feature instance where textContent attribute is present, and two or more information subAttributes are present, and the text subattributes are equal. | Values for text sub attribute are identical. | Ensure that text subattributes are populated with the correct values. | Logical consistency | B, U |
| 117 | For each feature instance where textContent attribute is present, and two or more information subAttributes are present, and the combination of fileReference and fileLocator subattributes are equal. | Values for file  reference and locator combinations are identical. | Ensure that national language attributes are populated with the correct values. | Logical consistency | B, U |
| 118 | For each featureName subattribute with language not equal to eng, and where featureName subattributes with language equal to eng is not present. | Name is encoded in national language only. | Populate text attribute with English text. | Logical consistency | B, U |
| 119 | For each information subattribute with language not equal to eng, and where information subattribute with language equal to eng is not present. | Text is encoded in national language only | Populate name attribute with English text. | Logical consistency | B, U |
| 120 | If the horizontalDatum reference and value attributes of DataSetDiscoveryMetadata are Not equal to EPSG:4326 (WGS 84). | horizontalDatum reference and value are not EPSG 4326 | Set the horizontalDatum reference and value attributes to EPSG 4326 | PS 8.1.1, 8.1.2 and 14.2 | B, U |
| 121 | If the file names in an exchange set are not in accordance with the Product Specification. | File names are not in accordance with the Product Specification. | Amend file names. | PS 11.4, 11.5 and 11.6 | B, U |
| 122 | For each feature instance that does not OVERLAP OR is WITHIN an area of dataCoverage | Object outside area of coverage. | Remove object or amend coverage. | PS 10.9  DCEG 2.6.3 | B, S |
| 123 | For each feature instance which does not have a valid feature class label/code as defined by the feature catalogue. | Object has invalid feature class code. | Amend object class code. | Logical consistency | B, U |
| 124 | For each attribute which does not have a valid attribute label/code as defined by the feature catalogue. | Attribute has invalid attribute label/code. | Amend attribute label/code. | Logical consistency | B, U |
| 125 | For each feature object which contains attributes outside the list of permissible attributes for the feature class (as defined in the feature catalogue). | Attribute not permitted on feature class. | Remove attribute. | Logical consistency | B, U |
| 126 | For each feature instance which is not COVERED\_BY the combined coverage of QualityOfNonBathymetricData meta feature instance. | Feature instance not covered by an QualityOfNonBathymetricData instance. | Ensure full coverage of QualityOfNonBathymetricData instance. | PS 10.11 | B, S |
| 127 | If the order of the data in a dataset is not correct. | Incorrect data order. | Amend data order. | PS 10.7.1 | B, U |
| 128 | For each attribute instance where the total number of instances exceed the permitted number of instances | Too many instances of attribute. | Ensure correct attribute encoding. | Logical consistency | B, U |
| 129 | For each feature instance where periodicDateRange subattributes dateEnd and dateStart are notNull AND their values are identical. | Object has identical values of periodicDateRange subattributes dateEnd and dateStart. | Ensure values of periodicDateRange subattributes dateEnd and dateStart are logical. | Logical consistency | B, U |
| 130 | For each feature instance where periodicDateRange subattribute dateStartis notNull AND dateEnd is Null OR not Present. | Object has dateStart without a value of dateEnd. | Populate dateEnd or remove dateStart. | Logical consistency | B, U |
| 131 | For each feature instance where periodicDateRange subattribute is notNull AND dateStart is Null OR not Present. | Object has dateEnd without a value of dateStart. | Populate dateStart or remove dateEnd. | Logical consistency | B, U |
| 132 | For each linear geometry which contains vertices at a density Greater than 0.3mm at 1:10000. | Vertex density exceeds the allowable tolerance. | Generalise edge(s). | PS 6.1 | B, U |
| 133 | For each instance of ServiceHours where an instance of scheduleByDayOfWeek attribute has temporal overlaps specified by timeIntervalByDayOfWeek attribute. | Time intervals within the same scheduleByDayOfWeek attribute overlap. | Review time intervals and remove time overlap. | Logical consistency | B, U |
| 134 | For each instance of ServiceHours with more than one instance of scheduleByDayOfWeek, and where an instance of scheduleByDayOfWeek has a temporal overlap with another instance of scheduleByDayOfWeek. | Schedule overlaps. | Review service hour intervals and remove time overlap. | Logical consistency | B, U |
| 135 | For each instance of a file referenced in the data and it is not present in the exchange set. | File referenced in the dataset is not present in the exchange set. | Add file to exchange set or remove reference to file. | PS 11.4 | B, S |
| 136 | For each instance of a dataset present in the exchange set and that does not have dataset discovery metadata. | Dataset discovery metadata is missing for dataset. | Add dataset discovery metadata. | PS 14.2, 14.3 | B, U |
| 137 | For each instance of a support file present in the exchange set and that does not have support file discovery metadata. | Support file discovery metadata is missing for support file. | Support file discovery metadata. | PS 14.3 | B, U |
| 138 | For each file referenced by the catalogue file in the exchange set and not present in the exchange set. | File is missing from exchange set. | Add file to exchange set or remove reference to file. | PS 14.5, 14.6 | B, U |
| 139 | For each feature instance which CROSS the 180° meridian. | Data crossing the 180° meridian. | Split the dataset along the 180° meridian. | DCEG 2.6.9 | B, U |
| 140 | For each dataset discovery metadata file that does not correspond to the dataset discovery metadata content table. | Dataset discovery metadata file that does not correspond to the dataset discovery metadata content table. | Ensure correct encoding of the discovery metadata file. | PS 14.2, 14.3 | B, U |
| 141 | For each support file discovery metadata file, does not correspond to the support file discovery metadata content table. | Support file discovery metadata file that does not correspond to the support file discovery metadata content table. | Ensure correct encoding of the support file metadata file. | PS 14.4 | B, U |
| 142 | For each catalogue file discovery metadata file that does not correspond to the catalogue file discovery metadata content table. | Catalogue file discovery metadata file that does not correspond to the catalogue file discovery metadata content table. | Ensure correct encoding of the catalogue metadata file. | PS 14.5 | B, U |
| 143 | For each fixedDateRange  where dateEnd and  dateStart are not Null and  dateEnd is less than or  equal to dateStart. | dateEnd less than  dateStart. | Amend values of  dateEnd or dateStart  accordingly. | Logical consistency | B, U |
| 144 | For each fixedDateRange  where both dateEnd and  dateStart are omitted or  Null. | FixedDateRange not  populated making the attribute meaningless. | Populate at least one  of dateEnd or dateStart. | Logical consistency | B, U |
| 145 | For each fixedDateRange  where dateEnd or  dateStart is not Null but the  year component is not  specified. | Year is required in  fixedDateRange  dates. | Populate year  component of dateStart  and dateEnd | Logical consistency | B, U |
| 146 | For each textContent  attribute where both  information and  onlineResource are  missing or null. | TextContent is not  populated with meaningful information. | Populate information or  onlineResource. | Logical consistency | B, U |
| 147 | For each information  attribute where both  fileReference and text subattributes  are missing or  null. | Information is not  populated with meaningful information. | Populate fileReference  or text attribute. | Logical consistency | B, U |
| 148 | For each sourceIndication  where the sub-attributes  are missing or null. | SourceIndication is  not populated with meaningful information. | Populate source  Indication. | Logical consistency | B, U |
| 149 | For each contactAddress  with all sub-attributes  either omitted or null. | Contact address is  not populated with meaningful information. | Populate at least one  sub-attribute of  contactAddress. | Logical consistency | B, U |
| 150 | For each frequencyPair  with  frequencyShoreStationTra  nsmits or  frequencyShoreStationRec  eives both sub-attributes  either omitted or null. | Frequency pair  frequency attributes  are not populated with meaningful information. | Populate at least one of  frequencyShoreStation  Transmits or  frequencyShoreStation  Receives. | Logical consistency | B, U |
| 151 | For each Regulations,  Restrictions,  Recommendations,  NauticalInformation with  both graphic and  textContent missing or null. | Regulations,  Restrictions,  Recommendations,  NauticalInformation  not populated. | Populate at least one of  graphic and  textContent. | Logical consistency | B, U |
| 152 | For each Applicability  without at least one of its  attributes populated. | Applicability is not  populated with meaningful information. | Populate at least one  attribute of Applicability. | Logical consistency | B, U |
| 153 | For each  NonStandardWorkingDay  with all of dateFixed,  dateVariable, and  information missing or null. | NonStandardWorkin  gDay not populated with meaningful information. | Populate at least one of  dateFixed,  dateVariable, and  information. | Logical consistency | B, U |
| 154 | For each ContactDetails  without at least one non  Null attribute. | ContactDetails not  populated with meaningful information. | Populate at least one  attribute of  ContactDetails. | Logical consistency | B, U |
| 155 | For each association  where the target is not in  the dataset. | Associated feature  or information type  not present. | Correct or remove the  association, or add the  missing feature or  information type. | Logical consistency | B, S |
| 158 | For each radiocommunications attribute where transmissionContent and categoryOfMaritimeBroadcast are encoded. | transmissionContent can only be encoded when categoryOfMaritimeBroadcast is not encoded. | Remove transmissionContent or add an additional radiocommunications attribute. | PS 6.2.1.3 | B, U |
| 159 | For each ContactDetails where radiocommunications attribute is present and communicationChannel, signalFrequency, or frequencyPair is not present. | communicationChannel, signalFrequency, or frequencyPair should be encoded in radiocommunications. | Encode communicationChannel, signalFrequency, or frequencyPair in radiocommunications. | PS 6.2.1.4 | B, U |
| 167 | If the update dataset file size is greater than 500Kbytes. | The update is larger than 500 KB in size. | Ensure that the cell is not larger than 500 Kbytes. | PS 11.2 | U |
| 168 | For each update dataset, a base dataset of the same dataset name is not either present on the system, in the same exchange set, or in another exchange set in the collection of exchange sets. | Base dataset not present. | Verify that the absence base dataset is not an error. | Logical consistency | U |
| 169 | For each update dataset with updateNumber N > 1, the base dataset is present and updates 1 to N-1 are not present on the system, in the exchange set, or in another exchange set on the system. | Preceding updates not present. | Obtain and install preceding updates. | Logical consistency | U |
| 170 | For each update dataset, without a feature, information type, or support file. | Empty update. | Add the data or support file or correct the metadata. | Logical consistency | U |
| 171 | For each cancellation (termination) of a dataset that does not exist on the system or has already been cancelled. | Terminated dataset is not present. | Ignore the update. | Logical consistency | U |
| 172 | For each cancellation (termination) of a dataset where the update exchange set contains a corresponding dataset file. | Cancellations cannot contain data objects. | Remove the dataset file from the exchange set or correct the metadata. | Logical consistency | U |
| 173 | For each RouteingMeasure with categoryOfRouteingMeasure ≠ 5 AND categoryOfTrafficSeparationScheme populated. | Category of TSS applies only to traffic separation schemes. | Remove the categoryOfTrafficSeparationScheme attribute. | PS 6.2.1.9 | B, U, S |
| 174 | For each UnderkeelClearanceManagementArea with dynamicResource = 2 or 3 and without an association to a ContactDetails object. | Features for dynamic resources must indicate a source for the dynamic information. | Add a ContactDetails object and associate the UKCM feature to it. | PS 6.2.1.12 | B, S |
| 175 | For each WaterwayArea with dynamicResource = 2 or 3 and without an association to a ContactDetails object. | Features for dynamic resources must indicate a source for the dynamic information. | Add a ContactDetails object and associate the WaterwayArea feature to it. | PS 6.2.1.12 | B, S |
| 176 | For each underkeelAllowance complex attribute without any of underkeelAllowance Fixed/Variable/BeamBased sub-attributes populated. | Underkeel allowance attribute is not populated. | Populate at least one of underkeelAllowance Fixed/Variable/BeamBased sub-attributes. | PS 6.2.1.12 | B, U |
| 177 | For each underkeelAllowance complex attribute without more than one of underkeelAllowance Fixed/Variable/BeamBased sub-attributes populated and operation not populated. | Underkeel allowance with more than one factor must specify how the factors are combined. | Populate sub-attribute operation. | PS 6.2.1.12 | B, U |
| 178 | For each RouteingMeasure with categoryOfRouteingMeasure ≠ 4 AND categoryOfNavigationLine populated. | Category of navigation line applies only to recommended tracks. | Remove the categoryOfNavigationLine attribute. | PS 6.2.1.9 | B, U, S |
| 179 | For each feature with more than one associated ContactDetails instance with call name attribute encoded AND that does not have different values in the language attribute. | Call name in different languages should be noted by the appropriate language. | Populate language | DCEG 7.9 | B, U, S |
| 180 | For each PilotService with more than one PilotDistrict associated via a serviceArea role. | PilotService can have at most one associated PilotDistrict service area associated. | Remove association to all but one of the associated PilotDistrict features. | DCEG 5.13 | B, U, S |

1. Data quality measures and reporting

Data quality measures should be reported using the ISO data quality schemas specified in ISO 19115-3, extended as necessary for S-100. Data quality elements recommended in the IHO data quality checklist and applicable to S-127 are listed in the product specification.

**Annex A**

1. Introduction
   1. ISO 19125-1:2004 geometry.

This clause defines ISO 19125-2004 geometric terms used in this Annex.

* + 1. Definitions for ISO 19125-1:2004 geometry

Note that these definitions are for the primitives defined by ISO 19125-1:2004 which are single point, single line, and single area geometry objects.

*Polygon* – A Polygon has a geometric dimension of 2. It consists of a boundary and its interior, not just a boundary on its own. It is a simple planar surface defined by 1 exterior boundary and 0 or more interior boundaries. The geometry used by an S-57 Area feature is equivalent to a Polygon.

*Polygon boundary* – A Polygon boundary has a geometric dimension of 1 and is equivalent to the outer and inner rings used by an S-57 Area feature.

* *LineString* – A LineString is a Curve with linear interpolation between Points. A LineString has a geometric dimension of 1. It is composed of one or more segments – each segment is defined by a pair of points. The geometry used by an S-57 Line feature is equivalent to a LineString.
* *Line* - An ISO 19125-1:2004 line is a LineString with exactly 2 points. Note that the geometry used by an S-57 Line feature is equivalent to a LineString, not a line in ISO 19125-1:2004 terms. In this document the term Line refers to an S-57 Line feature or a LineString which can have more than two points.
* *Point* – Points have a geometric dimension of 0. The geometry used by an S-57 Point feature is equivalent to an ISO 19125-1:2004 point.
* *Reciprocal* – inversely related or opposite.

The following table matches 19125-1:2004 geometric terms to S-57 terms:

|  |  |
| --- | --- |
| **ISO 19125-1:2004** | S-57 |
| Polygon | Area feature geometry OR Area |
| Polygon boundary | Outer and inner rings |
| LineString | Line feature geometry OR Line |
| Point | Point feature geometry OR Point |

* + 1. Definition of symbols used in ISO 19125-1:2004

I = interior of a geometric object

E = exterior of a geometric object

B = boundary of a geometric object

∩ = the set theoretic intersection

U = the set theoretic union

∧ = AND

Ú = OR

≠ = not equal

 = the empty or null set

**a** = first geometry, interior and boundary (the topological definition)

**b** = second geometry, interior and boundary (the topological definition)

dim = geometric dimension – 2 for Polygons , 1 for LineStrings, and 0 for Points

Dim(x) returns the maximum dimension (-1, 0, 1, or 2) of the geometric objects in x, with a numeric value of -1 corresponding to dim (Æ).

Note:

* Neither interior nor exterior include the boundary (i.e. I, E and B are mutually exclusive).
* The boundary of a Polygon includes its set of outer and inner rings.
* The boundary of a LineString is its end points except for a closed LineString, which has no boundary; the rest of the LineString is its interior.
* A Point does not have a boundary.
  1. ISO 19125-1:2004 geometric operator relationships

In ISO 19125-1:2004 (see Reference [1]), the dimensionally extended nine-intersection model (DE-9IM) defines 5 mutually exclusive geometric relationships between two objects (Polygons, LineStrings, and/or Points). One and only one relationship will be true for any two given objects (see Reference [2]):

1. WITHIN

2. CROSSES

3. TOUCHES

4. DISJOINT

5. OVERLAPS

There are others that help further define the relationship:

1. CONTAINS

* the reciprocal of WITHIN
* Within is the primary operator; however, if **a** is not within **b** then **a** may contain **b** so CONTAINS may be the unique relationship between the objects.

2. EQUAL

* a special case of WITHIN / CONTAINS.

3. INTERSECTS

* reciprocal of DISJOINT
* have at least one point in common

4. COVERS and is COVERED\_BY

* reciprocal operators
* extends CONTAINS and WITHIN respectively

5. COINCIDENT

Note that COVERS, COVERED\_BY, and COINCIDENT relational operators are not described in the ISO 19125-1:2004 document.

The formulas given in this annex (e.g. a.Disjoint(b) a b *=* ) are the generalized ones given for ISO 19125-1, not the more specific DE-9IM formulas (i.e. DE-9IM predicates). The generalized formulas use topologically closed notation (i.e. geometry includes the interior and boundary unless otherwise stated), whereas the DE-91M formulas refer to the interior and boundary of geometry separately. Note that different versions of documents describing 19125-1 give different generalized formulas – this annex is using the formulas that are the most consistent with the DE-9IM predicates. If a generalized formula appears to contradict a DE-9IM predicate as defined in ISO 19125-1:2004, the DE-9IM predicate takes precedence. Software is expected to be consistent with DE-9IM predicates.

* 1. How the relationships apply to S-57 Features

Geometric relationships will be tested on an entire S-57 feature object as a single geometric entity. Note that  S-57 Point, Line, and Area feature geometry is equivalent in ISO 19125-1:2004  terms to Point, LineString, and Polygon geometry respectively.

A Line feature in S-57 may be made up of several individual edges. The geometric relationship operators used with a Line feature will consider the sequence of edges as a single geometry (LineString).

A test on an Area feature will operate on the entire Polygon.

In an S-57 file a Line or Area feature may be split into pieces as a result of a cutting operation from a data source. In that case each feature record in the dataset is treated as a separate LineString or Polygon when testing geometric relationships.

If a test intends to operate only on a feature’s specific components – Polygon boundary (all rings), Polygon outer ring, Polygon inner rings, edges, vertices, or nodes then it must make this explicit in the description of the test. When a specific linear portion is specified in a test (Polygon boundary, edge) then it is treated as a LineString while individual vertices or points will be treated as points.

For example a test to look for cases where object class A OVERLAPS object class B would operate on the entire geometry. While a test to see if boundary of Area object class A OVERLAPS an edge of Line class B will be comparing Area boundaries to edges using Line to Line comparisons.

1. Geometric Operator Definitions

The ISO 19125-1 definitions referenced in this clause refer to clause 6.1.14.3 entitled “Named spatial relationship predicates based on the DE-9IM” in the ISO 19125-1:2004 document.

(In the diagrams within this annex LineString corresponds to the S-57 Line geometric primitive)

**EQUALS –** Geometric object **a** is spatially equal to geometric object **b**.

*The two geometric objects are the same. This is a special case of WITHIN.*



**Examples of the EQUALS relationship**

Note: ISO 19107:2003 describes equality more formally as:

Two different GM\_Objects are equal if they return the same Boolean value for the operation GM\_Object::contains for every tested DirectPosition within the valid range of the coordinate reference system associated to the object.

NOTE Since an infinite set of direct positions cannot be tested, the internal implementation of equal must test for equivalence between two, possibly quite different, representations. This test may be limited to the resolution of the coordinate system or the accuracy of the data. Application schemas may define a tolerance that returns true if the two GM\_Objects have the same dimension and each direct position in this GM\_Object is within a tolerance distance of a direct position in the passed GM\_Object and vice versa.

For the purposes of S-127 Validation Checks, a GM\_Object is any spatial object as described in A.1.1 (Polygons, LineStrings, and Points). A spatial object is always equal to itself, i.e., **a** EQUALS **a** is always true.

**DISJOINT –**  Geometric object **a** and geometric object **b** do not intersect.

*The two geometric objects have no common points.*

The ISO 19125-1 definition of DISJOINT is:

***a****.Disjoint(****b****)* ***a******b*** *=* 

This translates to: **a** is disjoint from **b** if the intersection of **a** and **b** is the empty set.



**Examples of the DISJOINT relationship**

**TOUCHES –** Geometric object **a** intersects with geometric object **b** but they do not share interior points.

*Only the boundary of one geometry intersects with the boundary or interior of another geometry.*

*The only thing the geometric objects have in common is contained in the union of their boundaries.*

The ISO 19125-1 definition of TOUCHES is:

***a****.Touch(****b****)* *(I(****a****)**I(****b****) =* *)* *(****a******b****)* 

This translates to: **a** touches **b** if the intersection of the interior of **a** and the interior of **b** is the empty set AND the intersection of **a** and **b** is not the empty set.

Note: This operator applies to the Area/Area, Line/Line, Line/Area, Point/Area, and Point/Line relationships. It does not apply to a Point/Point relationship since points do not have a boundary.



**Examples of the TOUCHES relationship.**

*Note the Polygon touches Polygon example (a) is also a case where the Polygon boundaries are COINCIDENT. In the Polygon/LineString example two of the LineStrings that share a linear portion of the Polygon boundary are also COINCIDENT with the Polygon boundary.*

**WITHIN** – Geometric object **a** is completely contained in geometric object **b**.

*WITHIN includes EQUALS.*

The definition of WITHIN is:

**a**. Within(**b**) ⇔ (**a** ∩ **b** = **a**) ∧ (I(**a**) ∩ I(**b**) ≠ )

This translates to: **a** is within **b** if the intersection of **a** and **b** equals **a** AND the intersection of the interior of **a** and the interior of **b** is not the empty set.

Note that this formula matches the one given in **the OpenGIS Simple Features Specification for SQL, Revision 1.1 (OpenGIS Project Document 99-049, Release Date: May 5, 1999**) which is the precursor to ISO 19125-1.

**Examples of the WITHIN relationship — Polygon/Polygon (a), Polygon/LineString (b), LineString/LineString (c), Polygon/Point (d), and LineString/Point (e)**

*Note that a Line that completely falls on a Polygon boundary is not WITHIN the Polygon, it TOUCHES it. In that case it would also be COINCIDENT with the Polygon boundary and COVERED\_BY the Polygon.*

**OVERLAPS -** The intersection of two geometric objects with the same dimension results in an object of the same dimension but is different from both of them.

*For two Polygons or two LineStrings, part of each geometry, but not all, is shared with the other.*

The OVERLAPS relationship is defined for Area/Area and Line/Line relationships. Points are either equal or disjoint.

*Note that this does not include lines that cross.*

The ISO 19125-1 definition of OVERLAPS is:

***a****.Overlaps(****b****)* *(dim(I(****a****)) = dim(I(****b****)) = dim(I(****a****)* *I(****b****)))* *(****a******b******a****)* *(****a******b******b****)*

This translates to: **a** OVERLAPS **b** if the geometric dimension of:

1. the interior of **a**
2. the interior of **b**
3. the intersection of the interiors of **a** and **b**

are all equal AND the intersection of **a** and **b** does not equal either **a** or **b**.



**Examples of the OVERLAPS relationship**

Note Lines that OVERLAP are also COINCIDENT.

**CROSSES –** The intersection of geometric object **a** and geometric object **b** returns geometry with a dimension less than the largest dimension between **a** and **b** but is not the same as geometric object **a** or **b**.

*Two LineStrings cross each other if they meet on an interior point. A LineString crosses a Polygon if the LineString is partly inside the Polygon and partly outside.*

The definition of CROSSES is:

***a****.Cross(****b****)*  *(I(****a****)* *I(****b****)* *)*  *(dim(I(****a****)* *I(****b****)) < max(dim(I(****a****)), dim(I(****b****))))* *(****a******b******a*** *)* *(****a******b******b****)*

This translates to: **a** crosses **b** if the intersection of the interiors of **a** and **b** is not the empty set AND the dimension of the result of the intersection of the interiors of **a** and **b** is less than the largest dimension between the interiors of **a** and **b** AND the intersection of **a** and **b** does not equal either **a** or **b**.

Note that “*(I(****a****)* *I(****b****)* *)* “ was added to the beginning of the ISO 19125-1 formula so that it would not be true for disjoint geometry.

The CROSSES operator only applies to Line/Line and Line/Area relationships.



**Examples of the CROSSES relationship**

*Note that example c) shows one solid line and one dashed line – their interiors intersect. If any Line were split into two separate Line features at the intersection point then the relationship would be TOUCHES because a boundary would be involved.*

**INTERSECTS** is the reciprocal of DISJOINT.

*The two geometric objects cross, overlap or touch, or one is within (or is contained by) the other. They have at least one common point.*

**CONTAINS** is the reciprocal of WITHIN.

*Given two geometric objects,* ***a*** *and* ***b****, if* ***a*** *is within* ***b*** *then* ***b*** *must contain* ***a****.*

**COVERED\_BY** (not a standard ISO 19125-1 operator)

No point of geometry **a** is outside geometry **b**.

The definition of COVERED\_BY is:

**a**. COVERED\_BY (**b**) ⇔ (**a** ∩ **b** = **a**)

This translates to: **a** is COVERED\_BY **b** if the intersection of **a** and **b** equals **a**.

The following expressions are equivalent to **a** is COVERED\_BY **b**:

1. Polygon (**a**) is COVERED\_BY Polygon (**b**): Polygon **a** is WITHIN a polygon **b** (WITHIN includes EQUALS)
2. Point (**a**) is COVERED\_BY Polygon (**b**): Point **a** is WITHIN or TOUCHES polygon **b**
3. Line (**a**) is COVERED\_BY Polygon (**b**): Line **a** is WITHIN polygon **b** or WITHIN the boundary of Polygon **b**
4. Line (**a**) is COVERED\_BY Line (**b**): Line **a** is WITHIN Line **b** (WITHIN includes EQUALS)
5. Point (**a**) is COVERED\_BY Line (**b**): Point **a** is WITHIN or TOUCHES Line **b**
6. Point (**a**) is COVERED\_BY Poiint (**b**): Point **a** EQUALS Point **b**

*Note that the figure below on the left is an example of Lines that are COVERED\_BY a polygon.*

*The figure on the right is NOT an example of a Line that is covered by a Polygon – it is an example of a Line that TOUCHES a Polygon. In both cases the Lines are COINCIDENT with the Polygon boundary.*



**Examples of COVERED\_BY and NOT COVERED\_BY**

**COVERS** (not a standard ISO 19125-1 operator)

COVERS is the reciprocal of COVERED\_BY.

*Given two geometric objects,* ***a*** *and* ***b****, if* ***a*** *is* COVERED\_BY ***b*** *then* ***b*** *must cover* ***a****.*

**COINCIDENT** (not an ISO 19125-1 operator)

Two geometric Lines OVERLAP or one geometric Line is WITHIN the other. Note that EQUAL Lines are also COINCIDENT by this definition.

*The intersection of two geometric Lines results in one or more Lines.*

This operator is only to be used to compare a Line with another Line. Note that normally the boundary of a Polygon is not the same as a Line but for this operation the boundary of a Polygon, exterior and interior rings, is treated as Lines for the COINCIDENT test.

The following expressions are equivalent to **a** is COINCIDENT with **b**:

1. Polygon (**a**) is COINCIDENT with Polygon (**b**): The boundary of Polygon **a** OVERLAPS or is WITHIN the boundary of Polygon **b**.

2. Line (**a**) is COINCIDENT WITH Polygon (**b**) : Line **a** OVERLAPS or is WITHIN the boundary of Polygon **b**.

3. Line (**a**) is COINCIDENT WITH Line (**b**): Line **a** OVERLAPS or is WITHIN Line **b**



**Example of two COINCIDENT geometric LINES**



**Examples of COINCIDENT objects**

Above are other examples of objects COINCIDENT with the boundary of a Polygon. LineStrings following a portion of a Polygon boundary or Polygons sharing a boundaryportion.

*Note that by definition a Line can be COINCIDENT with an interior boundary of a Polygon*.

*Note that other relationships may also be true, such as COVERED\_BY or TOUCHES, since COINCIDENT is not mutually exclusive.*

***Bibliography***

[1] ISO 19125-1:2004, *Geographic Information – Simple feature access – Part 1 Common architecture*

[2] CLEMENTINI, E., DI FELICE, P., VAN OOSTROM, P. *A Small Set of Formal Topological Relationships Suitable for End-User Interaction, in D. Abel and B. C. Ooi (Ed.), Advances in Spatial Databases* — Third International Symposium. SSD 1993. LNCS **692**, pp. 277-295. Springer Verlag. Singapore (1993)

[3] ISO 19107:2003, *Geographic information* *Spatial schema*

[4] OpenGIS Simple Features Specification for SQL, Revision 1.1*(OpenGIS Project Document 99-049, Release Date: May 5, 1999)*